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     CONFOCAL MICROSCOPY UNIT
ZEISS Axioscan 7

The ZEISS Axioscan 7 is an automated slide scanner designed for high-throughput imaging of biological samples. It supports brightfield, TIE contrast, and fluorescence imaging, enabling fast and reproducible digitization of slides for research and pathology workflows.

Features:
Imaging Modes
Brightfield and fluorescence imaging
Stage 
Motorized slide magazine with up to 100 slides
Detector 
Axiocam 705 color camera
Axiocam 712 monochrome camera

Objective lenses:
Magnification
Immersion
Type 
Numerical Aperture
Working Distance (mm)
5X
Air
Fluar
0.25
12.5
10X
Air
PlanApo
0.45
2.0
20X
Air
PlanApo
0.80

20x
Air
Plan-Neofluar
0.50
2.0
40x
Air
PlanApo
0.95


Laser module:
LED light source (Viluma 7)
Multiple filter sets (91 HE LED, 112 HE LED), with dedicated bandpass filter
Description 
Excitation (nm)
DAPI 
405
FITC 
488
TRIC 
561
Cy5
640
Cy7
750

Software: 
https://www.zeiss.com/microscopy/en/products/software/zeiss-zen-lite.html
Download Zen installer and follow the steps to install Zen Lite
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